FEMA CATEGORIES AND EXAMPLES OF COMMON ELIGIBLE WORK

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| A  | B  | C  | D  | E  | F  | G  |
| Debris Removal  | Emergency Protective Measures  | Roads & Bridges  | Water Control Facilities  | Buildings & Equipment  | Utilities  | Parks, Recreation, & Other  |
| Debris removal must be in the public interest and necessary to: * Eliminate immediate

threats to lives, public health & safety; * Eliminate immediate threats of significant damage to improved public or private property

Trees and Woody Debris Building Components Sand, Mud, Silt, & Gravel Removal of Temporary Levees   | Search & Rescue Security Emergency Pumping Sandbagging Detour & Warning Signs EOC Activation Emergency & Temporary Repairs Overhead Power Lines Emergency Medical Facilities Emergency Evacuations Activities undertaken before, during and following a disaster to save lives, protect improved property  | Roads * Surfaces
* Bases
* Shoulders
* Ditches
* Drainage

Structures * Low Water

Crossings Bridges * Decking & Pavement
* Piers
* Girders
* Abutments
* Slope Protection
* Approaches

Slope Failures  | Dams and Reservoirs Levees Engineered drainage Channels Canals Aqueducts Sediment Basins Shore Protective Devices Irrigation Facilities Pumping Facilities   | Buildings Structural Components Interior Systems * Electrical
* Mechanical
* Contents
 | Water Treatment Plants Power Generation & Distribution Facilities * Natural Gas Systems
* Wind Turbines
* Generators
* Substations
* Power Lines
 | Playground Equipment Swimming Pools Bath Houses Tennis courts Boat Docks Piers Picnic Tables Golf Courses Fish Hatcheries Mass Transit Facilities  |