FEMA CATEGORIES AND EXAMPLES OF COMMON ELIGIBLE WORK

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| A | B | C | D | E | F | G |
| Debris Removal | Emergency  Protective  Measures | Roads & Bridges | Water Control  Facilities | Buildings  &  Equipment | Utilities | Parks, Recreation,  & Other |
| Debris removal must be in the public interest and necessary to:   * Eliminate immediate   threats to lives, public health & safety;   * Eliminate immediate threats of significant damage to improved public or private property   Trees and Woody Debris  Building  Components  Sand, Mud, Silt, & Gravel  Removal of  Temporary Levees | Search & Rescue  Security  Emergency  Pumping  Sandbagging  Detour & Warning Signs  EOC Activation  Emergency &  Temporary Repairs  Overhead Power  Lines  Emergency Medical  Facilities  Emergency  Evacuations Activities undertaken before, during and following a disaster  to save lives, protect improved property | Roads   * Surfaces * Bases * Shoulders * Ditches * Drainage   Structures   * Low Water   Crossings  Bridges   * Decking & Pavement * Piers * Girders * Abutments * Slope Protection * Approaches   Slope Failures | Dams and  Reservoirs  Levees Engineered drainage Channels  Canals  Aqueducts  Sediment Basins  Shore Protective  Devices  Irrigation Facilities  Pumping Facilities | Buildings  Structural  Components  Interior Systems   * Electrical * Mechanical * Contents | Water Treatment  Plants  Power Generation  & Distribution  Facilities   * Natural Gas Systems * Wind Turbines * Generators * Substations * Power Lines | Playground  Equipment  Swimming Pools  Bath Houses  Tennis courts  Boat Docks  Piers  Picnic Tables  Golf Courses  Fish Hatcheries  Mass Transit  Facilities |